      \fitem{filter_min_t}(nim, n:numeric) replaces the image $y$ of
      each breakpoint by the min taken on a sequence made of the
      \code{n} previous and the \code{n} next images in addition to
      $y$.  See p.~\pageref{fct:filterMinT}. 

      %%% -------------------------------------------------------

