RHN Satellite Server 4.1.0: Installation Guide
Prev | Chapter 8. Maintenance | Next

# 8.9. Implementing PAM Authentication

As security measures become increasingly complex, administrators must be given tools that simplify their management. For this reason, RHN Satellite Server supports network-based authentication systems via Pluggable Authentication Modules (PAM). PAM is a suite of libraries that helps system administrators integrate the Satellite with a centralized authentication mechanism, thus eliminating the need for remembering multiple passwords.

RHN Satellite Server supports LDAP, Kerberos, and other network-based authentication systems via PAM. To enable the Satellite to use PAM and your organization's authentication infrastructure, complete the following tasks.

Set up a PAM service file (usually `/etc/pam.d/rhn-satellite`) and have the Satellite use it by adding the following line to `/etc/rhn/rhn.conf`:

    pam_auth_service = rhn-satellite

This assumes the PAM service file is named `rhn-satellite`.

To enable a user to authenticate against PAM, select the checkbox labeled Pluggable Authentication Modules (PAM). It is positioned below the password and password confirmation fields on the Create User page.

As an example, to authenticate against Kerberos one could put the following in `/etc/pam.d/rhn-satellite`:

    #%PAM-1.0
    auth        required      /lib/security/pam_env.so
    auth        sufficient    /lib/security/pam_krb5.so no_user_check
    auth        required      /lib/security/pam_deny.so
    account     required      /lib/security/pam_krb5.so no_user_check

Please note that changing the password on the RHN website changes only the local password on the RHN Satellite Server, which may not be used at all if PAM is enabled for that user. In the above example, for instance, the Kerberos password will not be changed.

Prev | Home | Next
Automating Synchronization | Up | Enabling Push to Clients