Package Products :: Package ZenStatus :: Module zenping |
[hide private]
[frames] | no frames]

# Module zenping

source code

Classes | [hide private]
PingCollectionPreferences
PerIpAddressTaskSplitter
TopologyUpdater This updates the link between a device and the topology.

Functions | [hide private]
findIp() | source code

Variables | [hide private]
| __doc__ = `"""zenp`...``
| log = `logging.getLogger("zen.zenping")`
| COLLECTOR_NAME = `"zenping"`
| TOPOLOGY_MODELER_NAME = `"topology_modeler"`
| TOPOLOGY_CORRELATOR_NAME = `"topology_correlator"`
| MAX_BACK_OFF_MINUTES = `20`
| MAX_IFACE_PING_JOBS = `10`

Variables Details | [hide private]

  ### __doc__ Value:
      """zenping

      Determines the availability of a IP addresses using ping (ICMP).

      """