Package Products :: Package ZenStatus :: Module PingTask |
[hide private]
[frames] | no frames]

# Module PingTask

source code

Classes | [hide private]
PingCollectionTask

Variables | [hide private]
| __doc__ = `"""PingT`...``
| log = `logging.getLogger("zen.zenping")`
| COLLECTOR_NAME = `"zenping"`
| TOPOLOGY_MODELER_NAME = `"topology_modeler"`
| MAX_BACK_OFF_MINUTES = `20`
| MAX_IFACE_PING_JOBS = `10`
| STATUS_EVENT = `{'eventClass': Status_Ping, 'component': 'zenpi`...``

Variables Details | [hide private]

  ### __doc__ Value:
      """PingTask

      Determines the availability of a IP addresses using ping (ICMP).

      """

  ### STATUS_EVENT Value:
      {'eventClass': Status_Ping, 'component': 'zenping', 'eventGroup': 'Pin
      g'}