Package Products :: Package DataCollector :: Module TelnetClient |
[hide private]
[frames] | no frames]

# Module TelnetClient

source code

Classes | [hide private]
| TelnetClientProtocol State-machine-based class for telnet
| TelnetClient Reactor code to start communications and invoke our telnet transport mechanism.
| FakePlugin Fake class to provide plugin instances for command-line processing.

Functions | [hide private]
integer |
check(hostname) Check to see if a device supports telnet | source code
buildOptions(parser=None, usage=None) Command-line telnet options | source code
list of FakePlugins |
commandsToPlugins(commands) The TelntClient class expects plugins. | source code
main() Test harness main() | source code

Variables | [hide private]
| __doc__ = `"""TelnetCli`...``
| log = `logging.getLogger("zen.TelnetClient")`
| defaultPromptTimeout = `10`
| defaultLoginRegex = `'ogin:.$'`
| defaultPasswordRegex = `'assword:'`
| defaultEnable = `False`
| defaultTermLength = `False`
| responseMap = `"WILL", "WONT", "DO", "DONT"`

Function Details | [hide private]

### check(hostname) | source code
Check to see if a device supports telnet Parameters: `hostname` (string) - name or IP address of device Returns: integer whether or not telnet port is available To Do: support alternate ports

### commandsToPlugins(commands) | source code
The TelntClient class expects plugins. Convert commands like 'ls a', 'ls b' to plugin instances. Duplicate commands will (eventually) be removed. This is used to support command-line arguments. Parameters: `commands` (list of strings) - list of commands from command-line Returns: list of FakePlugins list of commands, plugin-style

### main() | source code
Test harness main() Usage: python TelnetClient.py hostname[:port] comand [command] Each command must be enclosed in quotes (") to be interpreted properly as a complete unit.

Variables Details | [hide private]

  ### __doc__ Value:
      """TelnetClient

      TelnetClient is used by TelnetClient to issue commands to a machine
      and return their output over the telnet protocol.

      Device Tree Parameters are:

      zTelnetLoginTries - number of times to try login default: 1
      ...